RetroModem Bridge v3.5 - FujiNet Network Support
================================================

New in v3.5
- FujiNet TCP/Telnet listener on TCP 2323 by default
- Raw TCP mode
- UDP auto-discovery on UDP 2324
- RMB_DISCOVER_V1 / RMB_HERE_V1 discovery protocol
- Telnet IAC negotiation filtering
- Correct literal 0xFF escaping
- ANSI/VT100 and CP437 byte preservation
- One network client at a time with clean reconnect
- Existing serial/COM transport retained
- LAN address and FujiNet URL shown in RMB
- Copy address / Copy FujiNet URL buttons

First use
1. Run RetroModemBridge-v3.5.exe.
2. Enable Network Listener.
3. Keep Telnet mode, TCP 2323, UDP 2324.
4. Allow RetroModem Bridge through Windows Firewall on PRIVATE networks if prompted.
5. FujiTerm can connect to N:TELNET://<RMB-IP>:2323/.

Discovery request: RMB_DISCOVER_V1
Discovery reply:   RMB_HERE_V1|<computer-name>|2323
